Setting up to use your Canon iPF9000 with CLEAR FOCUS Aqueous Inkjet-compatible Perforated Window Films

This profile works with both the 1.5- and 2-mm hole size perforated window films.

Note this profile was built on a Canon iPF9000 series but should also work on the 8000 series. 

Instructions are shown for printing through Photoshop using the Canon Driver. 

Add the profile to the appropriate directory of your PC or Mac.

In Photoshop, after setting up your page size, select Print with Preview.
In the first screen you will see your print space selected, followed by another selection area where you are to select the iFP9K_Clr_FOCUS_12x12_6Pass.icc profile. 

(Note: If the profile doesn't show up, it's been placed in the wrong folder.) 

Then Select Print
In the next screen, select from the material list Adhesive Synthetic Paper.
Then, using the various menus, select Std 600 DPI_ 6Pass, No color adjustment and turn off the material cutter. 
(Note: The Canon printer will cut the material so you may choose to turn this option on.) 

Finally, select Print.